#-------------------------------------------------------------------------------
# This is a MicroStation V8 Sheet Size Definition file.
#
# Lines that begin with # are for descriptive comments.
#
# $Copyright: (c) 2015 Bentley Systems, Incorporated. All rights reserved. $
#-------------------------------------------------------------------------------
# The active sheetsizes.def file is used to control the available list of Sheet Sizes
# which are used to define the printable area for sheet models.
#
# The format of this file consists of one sheet size definition per line, where the
# format of each line is:
#
# Name;     Units;      Height; Width;      TopMargin;  LeftMargin;  BottomMargin;  RightMargin; UnitSystems
#
# Name:
# Used for display of the sheet size in the user interface.  Use the special value "_[SYSTEM]_"
# to indicate that the program should use the standard builtin name.
#
# Units:
# Controls the interpretation of the subsequent numeric values such as Height and Width.  True
# scale will be applied to all values.
#
#   Valid values for Units are:
#   1 Inches
#   2 Millimeters
#
# Heigth and Width:
# Control the corresponding dimensions of the sheet.
#
# TopMargin, LeftMargin, BottomMargin, and RightMargin:
# Control the corresponding margins that decrease the printable area within the sheet size defined
# by the Height and Width.  Negative values can be used for any of the margins to move the margins
# outside of the displayed paper.
#
# UnitSystems:
# Used to filter the list of sizes.  The user interface will typically use the active model's
# master units to control the visible sizes.  Only sizes that specify a system that matches 
# the system of the active model will be displayed.  Multiple systems can be specified.  If 
# 1,2,3 is specified then the size will not be filtered based on the system.
#
# For each line any content following '#' is ignored.
#
# NOTE: The Roll paper sizes can be used with any roll paper device. The height and width will
# emulate the size of the paper after it is cut.
#
# NOTE: The Cut Sheet sizes can be use be used with most sheet paper printers such that the margin
# is less than the maximum printable area that the printing device can produce.
#
# To customize this data make a copy of this file, place it within your configuration, and
# define the configuration variable MS_CUSTOMSHEETSIZEDEF with that location.
#
#-------------------------------------------------------------------------------
#  Modified by COP (JM 28.02.2019)
#-------------------------------------------------------------------------------
#
# MicroStation Standard Sheet Size Examples
#
#   Name              Units       Height      Width     TopMargin  LeftMargin  BottomMargin  RightMargin  UnitSystems
ISO A0+1800 ;	        2;	       841;        1800;     	0.00;       0.00;       0.00;       0.00;		2          #A0+1800
ISO A0+1600 ;	        2;	       841;        1600;      	0.00;       0.00;       0.00;       0.00;		2          #A0+1600
ISO A0+1400 ;	        2;	       841;        1400;      	0.00;       0.00;       0.00;       0.00;		2          #A0+1400
_[SYSTEM]_ ;            2;         841;       1189;         0.00;       0.00;       0.00;       0.00;       2          #ISOA0
_[SYSTEM]_ ;            2;         594;        841;         0.00;       0.00;       0.00;       0.00;       2          #ISOA1
_[SYSTEM]_ ;            2;         420;        594;         0.00;       0.00;       0.00;       0.00;       2          #ISOA2
_[SYSTEM]_ ;            2;         297;        420;         0.00;       0.00;       0.00;       0.00;       2          #ISOA3
_[SYSTEM]_ ;            2;         210;        297;         0.00;       0.00;       0.00;       0.00;       2          #ISOA4

