IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
File name: "Exemple_Terrain__OpenRoads_IFC4.ifc"
Time stamp: "2022-07-01T13:06:13"
Author: "Vincent.Rault"
Preprocessor: "OpenRoadsDesigner 10.10.21.04"
Originating system: "OpenRoadsDesigner 10.10.21.04"
Authorization: "Administrator"
Application: "OpenRoadsDesigner" version "10.10.21.04" by Organization "Bentley Software"

People and organizations
  Person "Vincent.Rault" of Organization (no name given)
  Owner history of Person "Vincent.Rault" of Organization (no name given) | application "OpenRoadsDesigner" version "10.10.21.04" by Organization "Bentley Software" | change ADDED | created 1656680773 (2022-07-01T13:06:13Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "2022_Grenoble_Terrain_Existant"
  IFCSITE "2022_Grenoble_Terrain_Existant" | elevation above sea level 0.0 | postal address USERDEFINED: "Address 1", "Address 2", "City/Town", "State/Region", "Postal Code", "Country"
    IFCBUILDING "Building" | reference height above sea level 0.0 | terrain above sea level 0.0 | postal address USERDEFINED: "Address 1", "Address 2", "City/Town", "State/Region", "Postal Code", "Country"
      IFCBUILDINGSTOREY "BSMT" | elevation 412.902 | description "Basement"
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | names: "MeshElement" | property sets: Géométrie, Quantités Civil, Objet, Couche de composants

Property sets
  Géométrie | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Surface (m²) = 6093100.37090823 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume (m³) = 0.0000010819262081 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Quantités Civil | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Surface de talus supérieure (m²) = 3046550.18545412 (IFCAREAMEASURE) [SQUARE_METRE]
    Surface plane (m²) = 2967879.20896721 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume (m³) = 0.0000010819262081 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Objet | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Définition d'objet = "Mesh\Corridors\Divers\PT_Divers_L" (IFCTEXT)
    Nom d'objet = "Composants\Structures\Structures_Surfacques\IFC_MNT, IFC_MNT" (IFCTEXT)
  Couche de composants | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Description = "" (IFCTEXT)
    PK de départ = "" (IFCTEXT)
    PK de fin = "" (IFCTEXT)