{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet 1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":52,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet 1","index":0,"n_rows":14,"n_cols":39,"rows_kept":14,"cut":false,"hidden":false,"merged":[[6,27,6,33],[6,34,6,36],[6,37,6,43],[6,19,6,23],[6,1,6,4],[6,7,6,11],[6,12,6,18],[6,24,6,26],[1,24,3,36],[1,41,1,43],[2,2,2,7],[2,8,2,13],[2,14,2,18],[3,2,3,7],[1,2,1,7],[1,8,1,13],[1,14,1,18],[1,21,1,23],[3,8,3,13],[3,14,3,18],[2,20,3,23]]}
[]
[null,"Project ID","Demo10",null,null,null,null,null,"Client",null,null,null,null,null,null,null,null,null,null,null,null,"Remarks",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Turnaround"]
[null,"Project Name","Rail Project",null,null,null,null,null,"Due Date",null,null,null,null,null,"2021-12-11"]
[null,"Schedule ID","Demo10_1",null,null,null,null,null,"Scheduled Date"]
[]
[]
[null,"Sample Details",null,null,null,null,null,"Classification",null,null,null,null,"Chemical / Concrete",null,null,null,null,null,null,"Compaction",null,null,null,null,"Compressibility",null,null,"Strength (Total)",null,null,null,null,null,null,"Shear Stregth (Effective Stress)",null,null,"Other"]
[null,"Location","Depth (m)","Number"," Type Number","Sampled Date","ramarks 1","Moisture Content","Atterberg 4 point","Particle Density by Gas Jar","Particle Density by Small Pyknometer","Particle Size Distribution","Organic Content","Loss On Ignition","Sulphate Total","Sulphate Water Gravimetric","ph","Chloride Content","Atterberg 4 Point","Compaction Light","Compaction Heavy","Compaction Vibrating Hammer","Moisture Condition Value","Moisture Condition Relationship","CBR","Consolidation","Swelling Pressure Test","Laboratory Vane Test","Small Direct Shearbox","Ring shear Test","Triaxial Quick Undrained","test pressures","Triaxial UU Multi Stage","Triaxial UU Multi Specimen","Consolidated Drained Triaxial Test","Consolidated Undrained Triaxial Test","Consolidated Undrained Triaxial Multistage"]
[null,"BH01",0,1,"B","2020-06-24","testing ",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,200]
[null,"BH01",0.5,2,"B","2020-06-24",null,1,1,null,null,1]
[null,"BH02",0.25,1,"D","2020-06-24",null,1]
[null,"BH02",0.65,2,"U","2020-06-24",null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,"BH03",0.1,1,"B",null,null,2,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,500]
[null,"BH04",1,1,"B"]