LOAD 1 LOADTYPE Dead TITLE LOAD CASE 1 - DEAD

SELFWEIGHT Y -1.1 LIST 20 TO 34

MEMBER LOAD

97 114 116 TO 126 UNI GY -2.5

LOAD 2 LOADTYPE Roof Live TITLE LOAD CASE 2 - ROOF LIVE

MEMBER LOAD

53 TO 63 116 TO 126 UNI GY -50

LOAD 3 LOADTYPE Snow TITLE LOAD CASE 3 - SNOW

MEMBER LOAD

53 TO 56 116 TO 119 UNI GY -200

LOAD 4 LOADTYPE Wind TITLE LOAD CASE 4 - WIND PL+

MEMBER LOAD

124 TO 126 UNI Y 32

PMEMBER LOAD

1 UNI GX 86

2 UNI GX 96

LOAD 5 LOADTYPE Wind TITLE LOAD CASE 5 - WIND PL-

MEMBER LOAD

124 TO 126 UNI Y -32

PMEMBER LOAD

1 UNI GX 150

2 UNI GX 32